Neonode zForce(TM) SDK

Public Attributes | List of all members
EnableMessage Struct Reference

This structure represents an enable message. More...

`#include <EnableMessage.h>`

## Public Attributes
MessageType | MessageType
MessageGroup | MessageGroup
bool | Error
int | ErrorCode
uint64_t | SerialNumber
void(* | Destructor )(Message *self)
bool | Enabled
| True when device is enabled.
bool | ContinuousMode
| True when device is set to Continuous Mode.
uint32_t | NumberOfMessages
| Number Of Messages.

## Detailed Description

This structure represents an enable message.

This structure represents a message which indicates if the scanning on a device is turned on and if it is continous or has a defined number of messages to send set.

## Member Data Documentation

## ◆ Destructor

void( * EnableMessage::Destructor) (Message *self)

Destructor.
Inherited from Message base class.

## ◆ Error

bool EnableMessage::Error

If an error occurred, this is True.
Inherited from Message base class.

## ◆ ErrorCode

int EnableMessage::ErrorCode

Error Code, valid when Error == true.
Inherited from Message base class.

## ◆ MessageGroup

MessageGroup EnableMessage::MessageGroup

The Message Group of the Message.
Inherited from Message base class.

## ◆ MessageType

MessageType EnableMessage::MessageType

The Message Type of the Message.
Inherited from Message base class.

## ◆ SerialNumber

uint64_t EnableMessage::SerialNumber

Unique serial number for this message.
Inherited from Message base class.

The documentation for this struct was generated from the following file:

- EnableMessage.h