Neonode zForce(TM) SDK

Public Attributes | List of all members
TouchActiveArea Struct Reference

This structure represents the Touch Active Area of a sensor. More...

`#include <zForceTypes.h>`

## Public Attributes
uint32_t | LowerBoundX
| Start of the Touch Active Area X axis.
uint32_t | UpperBoundX
| End of the Touch Active Area X axis.
bool | HasX
| True if the coordinate system has a X axis.
uint32_t | LowerBoundY
| Start of the Touch Active Area Y axis.
uint32_t | UpperBoundY
| End of the Touch Active Area Y axis.
bool | HasY
| True if the coordinate system has a Y axis.

## Detailed Description

This structure represents the Touch Active Area of a sensor.

This structure represents the Touch Active Area of a sensor. The Touch Active Area is the area which a sensor will report touches from.

The documentation for this struct was generated from the following file:

- zForceTypes.h