Neonode zForce(TM) SDK

Public Attributes | List of all members
TouchActiveAreaMessage Struct Reference

This structure represents a touch active area message. More...

`#include <TouchActiveAreaMessage.h>`

## Public Attributes
MessageType | MessageType
MessageGroup | MessageGroup
bool | Error
int | ErrorCode
uint64_t | SerialNumber
void(* | Destructor )(Message *self)
uint32_t | LowerBoundX
| Start of the Touch Active Area X axis.
uint32_t | UpperBoundX
| End of the Touch Active Area X axis.
bool | HasX
| True when LowerBoundX and UpperBoundX are valid.
uint32_t | LowerBoundY
| Start of the Touch Active Area Y axis.
uint32_t | UpperBoundY
| End of the Touch Active Area Y axis.
bool | HasY
| True when LowerBoundY and UpperBoundY are valid.

## Detailed Description

This structure represents a touch active area message.

This structure represents a message which indicates what touch active area a device uses.

## Member Data Documentation

## ◆ Destructor

void( * TouchActiveAreaMessage::Destructor) (Message *self)

Destructor.
Inherited from Message base class.

## ◆ Error

bool TouchActiveAreaMessage::Error

If an error occurred, this is True.
Inherited from Message base class.

## ◆ ErrorCode

int TouchActiveAreaMessage::ErrorCode

Error Code, valid when Error == true.
Inherited from Message base class.

## ◆ MessageGroup

MessageGroup TouchActiveAreaMessage::MessageGroup

The Message Group of the Message.
Inherited from Message base class.

## ◆ MessageType

MessageType TouchActiveAreaMessage::MessageType

The Message Type of the Message.
Inherited from Message base class.

## ◆ SerialNumber

uint64_t TouchActiveAreaMessage::SerialNumber

Unique serial number for this message.
Inherited from Message base class.

The documentation for this struct was generated from the following file:

- TouchActiveAreaMessage.h