Neonode zForce(TM) SDK

Public Attributes | List of all members
ReverseTouchActiveAreaMessage Struct Reference

This structure represents a reverse touch active area message. More...

`#include <ReverseTouchActiveAreaMessage.h>`

## Public Attributes
MessageType | MessageType
MessageGroup | MessageGroup
bool | Error
int | ErrorCode
uint64_t | SerialNumber
void(* | Destructor )(Message *self)
bool | XIsReversed
| True if the X axis is reversed.
bool | YIsReversed
| True if the Y axis is reversed.

## Detailed Description

This structure represents a reverse touch active area message.

This structure represents a message which indicates what reverse touch active area a device uses.

## Member Data Documentation

## ◆ Destructor

void( * ReverseTouchActiveAreaMessage::Destructor) (Message *self)

Destructor.
Inherited from Message base class.

## ◆ Error

bool ReverseTouchActiveAreaMessage::Error

If an error occurred, this is True.
Inherited from Message base class.

## ◆ ErrorCode

int ReverseTouchActiveAreaMessage::ErrorCode

Error Code, valid when Error == true.
Inherited from Message base class.

## ◆ MessageGroup

MessageGroup ReverseTouchActiveAreaMessage::MessageGroup

The Message Group of the Message.
Inherited from Message base class.

## ◆ MessageType

MessageType ReverseTouchActiveAreaMessage::MessageType

The Message Type of the Message.
Inherited from Message base class.

## ◆ SerialNumber

uint64_t ReverseTouchActiveAreaMessage::SerialNumber

Unique serial number for this message.
Inherited from Message base class.

The documentation for this struct was generated from the following file:

- ReverseTouchActiveAreaMessage.h