Neonode zForce(TM) SDK

Public Attributes | List of all members
TouchModeMessage Struct Reference

This structure represents a touch mode message. More...

`#include <TouchModeMessage.h>`

## Public Attributes
MessageType | MessageType
MessageGroup | MessageGroup
bool | Error
int | ErrorCode
uint64_t | SerialNumber
void(* | Destructor )(Message *self)
TouchModes | TouchMode
| Touch Mode.
bool | HasTouchMode
| True when TouchMode is valid.
uint32_t | ClickOnTouchTime
| How long to wait for before a touch is clicked in Click on Touch Mode.
bool | HasClickOnTouchTime
| True when ClickOnTouchTime is valid.
uint32_t | ClickOnTouchRadius
| How far the touch has to move before it is switched to Normal Mode.
bool | HasClickOnTouchRadius
| True when ClickOnTouchRadius is valid.

## Detailed Description

This structure represents a touch mode message.

This structure represents a message that decides the touch mode.

## Member Data Documentation

## ◆ Destructor

void( * TouchModeMessage::Destructor) (Message *self)

Destructor.
Inherited from Message base class.

## ◆ Error

bool TouchModeMessage::Error

If an error occurred, this is True.
Inherited from Message base class.

## ◆ ErrorCode

int TouchModeMessage::ErrorCode

Error Code, valid when Error == true.
Inherited from Message base class.

## ◆ MessageGroup

MessageGroup TouchModeMessage::MessageGroup

The Message Group of the Message.
Inherited from Message base class.

## ◆ MessageType

MessageType TouchModeMessage::MessageType

The Message Type of the Message.
Inherited from Message base class.

## ◆ SerialNumber

uint64_t TouchModeMessage::SerialNumber

Unique serial number for this message.
Inherited from Message base class.

The documentation for this struct was generated from the following file:

- TouchModeMessage.h